**Alpha 20**

|  |  |  |
| --- | --- | --- |
| **Ordering information****Product Code AP20-****System Type 3 Ph. (PR. 3W or 4W)**\* System Type is Site selectable. 1 Ph.\*\* Select code for factory default setting.Input Voltage 100 TO 500VL-LInput Current 1/5APower Supply Self Aux40 V – 300 U12-48 V DCLimit switch With Limit switch Without Limit switchRS 485 With RS 485Without RS 485 | **X X X XX** | **X X 000000** |
| 3 |  |
| 1 |  |
| 1 |  |
| 1 |  |
| SA |  |
| EA |  |
| LA |  |
|  | L |
|  | Z |
|  | R |
|  | Z |