**P17G**

**P17G- Passive Separator**

|  |  |  |  |
| --- | --- | --- | --- |
| **Product Code** | **P17G-** | **XX** | **X** |
| **Version** | Standard | 00 |  |
| On Order\* | XX |  |
| **Acceptance Tests** | Without Additional Requirements |  | 8 |
| With a Quality Inspection Certificate |  | 7 |
| Acc. to Customer’ s Agreement\* |  | X |

**Commonly Used Ranges for P17G-**

Inp: 0/4-20mA DC; O/P: 0/4-20mA DC

P17G 00U0