**P18D**

**P18D- Temperature and Humidity Transducer with External Sensor**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Product Cod e** | **P18D-** | **X** | **XX** | **X** | **X** |
| **Analog Outputs** | Without Analog Outputs | 0 |  |  |  |
| Current 4 ... 20 mA | 1 |  |  |  |
| Voltage 0 ... 10 V | 2 |  |  |  |
| **Version** | Standard |  | 00 |  |  |
| On Order\* |  | XX |  |  |
| **Language** | Polish |  |  | P |  |
| English |  |  | E |  |
| Other |  |  | X |  |
| **Acceptance Tests** | Without Additional Requirements |  |  |  | 8 |
| With a Quality Inspection Certificate |  |  |  | 7 |
| Acc. to Customer’s Agreement\* |  |  |  | X |

**Commonly Used Ranges for P18D-**

|  |  |
| --- | --- |
| P18D 100U0 | Aux: 9-24VAC/DC; O/P: RS485 & 2x 4-20mA with Sensor on Housing |
| P18D 400U0 | Aux: 9-24VAC/DC; O/P: RS485 & 2x 4-20mA with Sensor on 0.5m Wire |