**RE57**

**TC40 – Basic Series Single Channel Temperature Controller (48X48, 96X96,48X96)**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Product Code** | **TC40-** | **X** | **XX** | **XX** | **X** | **XXXXX** | **XX** |
| **Size** | RE57 - 48X48 | A |  |  |  |  |  |
| RE96 - 96x96 | B |  |  |  |  |  |
| RE77 - 48X96 | C |  |  |  |  |  |
| **Output 1** | Relay |  | RL |  |  |  |  |
| SSR |  | SR |  |  |  |  |
| **Output 2** | Relay |  |  | RL |  |  |  |
| SSR |  |  | SR |  |  |  |
| None |  |  | 0 |  |  |  |
| **Power Supply** | 60-280 VAC/DC |  |  |  | H |  |  |
| 20-60VDC / 20-40VAC |  |  |  | L |  |  |
| **Version** | Standard |  |  |  |  | 00000 |  |
| **Brand** | STI |  |  |  |  |  | ST |