**Theta 60M**

**Theta 60M- Universal Transmitter**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Product Code** | **TT62-** | **X** | **X** | **X** | **X** | **X** | **XXXXXXXX** |
| **Current Input Range** | 1 A (X/1) | 1 |  |  |  |  |  |
| 5 A (X/5) | 2 |  |  |  |  |  |
| **Voltage Input Range** | 3Ph 57.7/100V |  | 1 |  |  |  |  |
| 3Ph 230/400V |  | 2 |  |  |  |  |
| **Supply Voltage** | 85 253 V a.c., 90..320V d.c |  |  | 1 |  |  |  |
| 20...40 V a.c..,20..60V d.c |  |  | 2 |  |  |  |
| **Output type** | without analog o/p 4 relays |  |  |  | 1 |  |  |
| 2 analog o/p, 2 relays |  |  |  | 2 |  |  |
| 4 analog o/p, without relays |  |  |  | 3 |  |  |
| **Load resistance (RL )** | 250 Ohm |  |  |  |  | 1 |  |
| 750 Ohm |  |  |  |  | 2 |  |
| **Version** | Standard |  |  |  |  |  | 00000000 |

**Commonly Used Ranges for Theta 60M-**

|  |  |
| --- | --- |
| TT62-1F00000000000 | V604; Cold Junction; Aux: 24-60VACDC |
| TT62-1J00000000000 | V604; Cold Junction; Aux: 85-230VACDC |