**ND40**

**ND40- Power Quality Analyzer with Ethernet**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Product Code** | **ND40-** | **X** | **X** | **XX** | **X** | **X** |
| **Analyzer/Recorder** | Class S | 0 |  |  |  |  |
| Class A/S | 1 |  |  |  |  |
| **Inputs / Outputs** | Without |  | 0 |  |  |  |
| 8 Relay Outputs |  | 1 |  |  |  |
| 6 Logic Inputs, 4 Relay Outputs |  | 2 |  |  |  |
| 6 Logic Inputs, 3 Analog Outputs |  | 3 |  |  |  |
| **Version** | Standard |  |  | 00 |  |  |
| Voltage Input 3 X 57.7/ 100V |  |  | 01 |  |  |
| Custom-Made |  |  | XX |  |  |
| **Language** | English |  |  |  | E |  |
| Other\* |  |  |  | X |  |
| **Acceptance Tests** | Without Additional Quality Requirements |  |  |  |  | 0 |
| With An Extra Quality Inspection Certificate |  |  |  |  | 1 |
| Acc.To Customer's Request\* |  |  |  |  | X |

**Commonly Used Codes for ND40-**

|  |  |
| --- | --- |
| ND40 1000U1 | Meas. Class: Class A/S; |
| ND40 1100U1 | Meas. Class: Class A/S; O/P: 8x Relay; |
| ND40 1200U1 | Meas. Class: Class A/S; Dig I/P: 6x Log; O/P: 4x Relay; |
| ND40 1300U1 | Meas. Class: Class A/S; Dig I/P: 6x Log; O/P: 3x Analog; |
| ND40 0000U1 | Meas. Class: Class S; |
| ND40 0100U1 | Meas. Class: Class S; O/P: 8x Relay; |
| ND40 0200U1 | Meas. Class: Class S; Dig I/P: 6x Log; O/P: 4x Relay; |
| ND40 0300U1 | Meas. Class: Class S; Dig I/P: 6x Log; O/P: 3x Analog; |