**Alpha 20**

|  |  |  |
| --- | --- | --- |
| **Ordering information**  **Product Code AP20-**  **System Type 3 Ph. (PR. 3W or 4W)**  \* System Type is Site selectable. 1 Ph.  \*\* Select code for factory default setting.  Input Voltage 100 TO 500VL-L  Input Current 1/5A  Power Supply Self Aux  40 V – 300 U  12-48 V DC  Limit switch With Limit switch Without Limit switch  RS 485 With RS 485  Without RS 485 | **X X X XX** | **X X 000000** |
| 3 |  |
| 1 |  |
| 1 |  |
| 1 |  |
| SA |  |
| EA |  |
| LA |  |
|  | L |
|  | Z |
|  | R |
|  | Z |