**Theta 40**

**Theta 40- Multifunction Transducer**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Product Code** | **TT40-** | **X** | **X** | **XXXXXXXXXXX** |
| **Product Type** | M42 | 1 |  |  |
| M24 | 2 |  |  |
| M20 | 3 |  |  |
| M40 RS 485 | 4 |  |  |
| M30 | 5 |  |  |
| M01 RS 485 | 6 |  |  |
| M00 LONBUS | 7 | F |  |
| **Power Supply** | 24-60V AC/DC |  |
| 85-230V AC/DC |  | J |  |
| **Version** | Standard |  |  | 00000000000 |

**Commonly Used Ranges for Theta 40-**

|  |  |
| --- | --- |
| TT40-1F00000000000 | Multi transducer: M42 Aux: 24-60VACDC; 4 Analog; 2 Digital; RS232 Interface |
| TT40-1J00000000000 | Multi transducer: M42 Aux: 85-230VACDC; 4 Analog; 2 Digital; RS232 Interface |
| TT40-2F00000000000 | Multi transducer: M24 Aux: 24-60VACDC; 2 Analog; 4 Digital; RS232 Interface |
| TT40-2J00000000000 | Multi transducer: M24 Aux: 85-230VACDC; 2 Analog; 4 Digital; RS232 Interface |
| TT40-3J00000000000 | Multi transducer: M20 Aux: 85-230VACDC; 2 Analog Outputs; RS 232 Interface |
| TT40-5J00000000000 | Multi transducer: M30 Aux: 85-230VACDC; 3 Analog Outputs; RS 232 Interface |
| TT40-4J00000000000 | Multi transducer: M40 RS485 Aux: 85-230VACDC; 4 Analog Outputs; RS 485 Interface |
| TT40-4F00000000000 | Multi transducer: M40 RS485 Aux: 24-60VACDC; 4 Analog Outputs; RS 485 Interface |