**N43**

**N43- Rail Mounted Power Network Meter**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Product Code** | **N43-** | **X** | **X** | **X** | **XX** | **X** | **X** |
| Current Input In | 1 A/ 5 A (X/1; X/5) 1 | |  |  |  |  |  |
| 63 A 2 | |
| Voltage Input (Phase/ Phase-To-Phase) Un | 3 X 57.7/ 100V | | 1 |
| 3 X 230/ 400V | | 2 |
| 3 X 290/ 500V | | 3 |
| Auxiliary Supply | 85 - 253V AC, 90 - 300V DC | | | 1 |
| 20 - 40V AC, 20 - 60V DC | | | 2 |
| Version | Standard | | | | 00 |
| Custom-Made\* | | | | XX |
| Language | English | | | | | U |
| Other\* | | | | | X |
| Acceptance Tests | Without Extra Quality Requirements | | | | | | 0 |
| With an Extra Quality Inspection Certificate | | | | | | 1 |
| Acc. to Customer’s Request\* | | | | | | X |

\* After agreeing with the manufacturer

**Commonly used codes For N43-**

|  |  |
| --- | --- |
| N43 11100U1 | I/P: 1/5A & 100V; Aux: 85…253V ACDC; 3 Relay Outputs; 1 Pulse Output; RS 485 Output; USB Port; DIN Rail Mounting |
| N43 13100U1 | I/P: 1/5A & 500V; Aux: 85…253V ACDC; 3 Relay Outputs; 1 Pulse Output; RS 485 Output; USB Port; DIN Rail Mounting |
| N43 21100U1 | I/P: 63A & 100V; Aux: 85…253V ACDC; 3 Relay Outputs; 1 Pulse Output; RS 485 Output; USB Port; DIN Rail Mounting |
| N43 23100U1 | I/P: 63A & 500V; Aux: 85…253V ACDC; 3 Relay Outputs; 1 Pulse Output; RS 485 Output; USB Port; DIN Rail Mounting |
| N43 11200U1 | I/P: 1/5A & 100V; Aux: 20…40V ACDC; 3 Relay Outputs; 1 Pulse Output; RS 485 Output; USB Port; DIN Rail Mounting |
| N43 13200U1 | I/P: 1/5A & 500V; Aux: 20…40V ACDC; 3 Relay Outputs; 1 Pulse Output; RS 485 Output; USB Port; DIN Rail Mounting |
| N43 21200U1 | I/P: 63A & 100V; Aux: 20…40V ACDC; 3 Relay Outputs; 1 Pulse Output; RS 485 Output; USB Port; DIN Rail Mounting |
| N43 23200U1 | I/P: 63A & 500V; Aux: 20…40V ACDC; 3 Relay Outputs; 1 Pulse Output; RS 485 Output; USB Port; DIN Rail Mounting |