**Omicron PHR**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Product Code** | **PR10-** | **X** | **X** | **X** | **X** | **X** | **X** | **0** | **0** | **0** | **0** | **0ST** |
| Model type for PR10 | Phase monitor relay | P |  |  |  |  |  |  | 0 | 0 | 0 | 0ST |
| System Type for PR10 | 3P3W |  | 4 |
| 3P4W |  | 5 |
| System Voltage for PR10 | 110VLL |  |  | 1 |
| 240VLL |  |  | 2 |
| 415VLL |  |  | 3 |
| 440VLL |  |  | 4 |
| System Freq for PR10 | 50Hz |  |  |  | 1 |
| 60Hz |  |  |  | 2 |
| Relay Configuration for PR10 | Normally Energized |  |  |  |  | 1 |
| Normally De-energized |  |  |  |  | 2 |
| No. of Relay for PR10 | 1 relay |  |  |  |  |  | 1 |
| Reserved | 0 | | | | | | | |