**Alpha 10**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Product Code** | **AP10-** | **X** | **X** | **X** | **XX** | **X** | **0000000** |
| Display Type | 3 Line | 3 |  |  |  |  |  |
| 1 Line (20mm display) | 1 |
| System Type | 3 Ph. (PR. 3W or 4W) |  | 3 |
| 1 Ph. |  | 1 |
| Input Voltage / Current | 100 TO 500VL-L 1/5A |  |  | 1 |
| Power Supply | \*Self Aux |  |  |  | SA |
| 40 V – 300 U |  |  |  | EA |
| 12-48 V DC |  |  |  | LA |
| Limit switch | \* With Limit switch |  |  |  |  | L |
| Without Limit switch |  |  |  |  | Z |