**Zeta 20**

**ZT20 - 1KV Digital Insulation & Continuity Tester, Insulation Resistance 2GW**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Product Code** | **ZT20-** | **X** | **X** | **X** | **XXXXXXXXXX** |
| **Product Type** | Zeta 20 | 1 |  |  |  |
| Zeta 20 Adapter Zeta20A | 2 |  |  |  |
| Zeta 20 with carrying case | 3 | N |  |  |
| **Cable set** | Normal |  |
| Fin Tip |  | F | E |  |
| **Cable Length** | Normal with 10 meter cab.10M |  |  |
| STD |  |  | S | 0000000000 |
| **Version** | Standard |

**Commonly Used Ranges for ZT20-**

|  |  |
| --- | --- |
| ZT20-1NS0000000000 | Zeta 20: Battery Operated, 1kV, 2Gohm, Hand held |
| ZT20-1FS0000000000 | Zeta 20: Battery Operated & Fine Tip, 1kV, 2GΩ |