**Zeta 50,50K**

**ZT50/50K – 5KV High Voltage Insulation Tester, Insulation Resistance 1TW**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Product Code** | **ZT50-** | **X** | **X** | **X** | **XXXXXXXXXX** |
| **Product Type** | Zeta 50A | 1 |  |  |  |
| Zeta 50AK | 2 |  |  |  |
| Zeta 50AKM | 3 |  |  |  |
| Zeta 50AKMR | 4 | N |  |  |
| **Cable set** | Normal |  |  |  |
| Fin Tip |  | B | S |  |
| **Cable Length** | STD |  |  |
| 1.5M |  |  | C |  |
| 2.0M |  |  | D |  |
| 2.5M |  |  | E |  |
| 3.0M |  |  | F |  |
| 3.5M |  |  | G |  |
| 4.0M |  |  | H |  |
| 5.0M |  |  | I |  |
| 6.0M |  |  | J |  |
| 6.5M |  |  | K |  |
| 8.0M |  |  | L |  |
| 8.5M |  |  |  | M |  |
| 10M |  |  | N |  |
| 15M |  |  | P |  |
| **Version** | Standard | 0000000000 |

**Commonly Used Ranges for Zeta 50-**

|  |  |
| --- | --- |
| ZT50-2NS0000000000 | Zeta 50: STD High Voltage Insulation Tester (5kV, 1TΩ) with hand crank generator operation |
| ZT50-1NS0000000000 | Zeta 50: STD High Voltage Insulation Tester (5kV, 1TΩ) with Battery Operation |