**NA3**

**NA3-Single Channel Vertical Multicolor Bar graph**

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Product Code** | **NA3-** | **X** | **X** | **X** | **X** | **X** | **X** | **X** | **X** | **XX** | **X** |
| **Meter Version** | With a Bargraph And Digital Display | F |  |  |  |  |  |  |  |  |  |
| With a Bargraph\* | B |  |  |  |  |  |  |  |  |  |
| With a Digital Display | D |  |  |  |  |  |  |  |  |  |
| **Bargraph Colour** | Without Bargraph (NA3D) |  | 0 |  |  |  |  |  |  |  |  |
| 3-Colour Bargraph (R, G, R+G) |  | T |  |  |  |  |  |  |  |  |
| 7-Colour Bargraph  (R, G, B, R+G, R+B, G+B, R+G+B) |  | M |  |  |  |  |  |  |  |  |
| **Display Colour** | Without Display |  |  | 0 |  |  |  |  |  |  |  |
| Red |  |  | R |  |  |  |  |  |  |  |
| Green |  |  | G |  |  |  |  |  |  |  |
| Blue |  |  | B |  |  |  |  |  |  |  |
| **Input Signal** | Universal Input |  |  |  | U |  |  |  |  |  |  |
| **Analog Output Signal** | Lack |  |  |  |  | 0 |  |  |  |  |  |
| Current Programmable 0/4...20 mA |  |  |  |  | 1 |  |  |  |  |  |
| Voltage Programmable 0...10 V |  |  |  |  | 2 |  |  |  |  |  |
| **Additional Output** | Lack\* |  |  |  |  |  | 0 |  |  |  |  |
| RS485 Digital Output + 1 Relay |  |  |  |  |  | 1 |  |  |  |  |
| RS485 Digital Output + 1 Output Of OC Type |  |  |  |  |  | 2 |  |  |  |  |
| 2 Relays\* |  |  |  |  |  | 3 |  |  |  |  |
| 2 Outputs Of OC Type\* |  |  |  |  |  | 4 |  |  |  |  |
| **Supply** | 95 ... 253 V AC/ DC |  |  |  |  |  |  | 1 |  |  |  |
| 20 ... 40 V AC/ DC |  |  |  |  |  |  | 2 |  |  |  |
| On Order\*\* |  |  |  |  |  |  | X |  |  |  |
| **Kind Of Terminals** | Socket-Screw Plug |  |  |  |  |  |  |  | 0 |  |  |
| **Version** | Standard |  |  |  |  |  |  |  |  | 00 |  |
| Custom-Made\*\* |  |  |  |  |  |  |  |  | XX |  |
| **Acceptance Tests** | Without An Extra Quality Inspection Certificate |  |  |  |  |  |  |  |  |  | 8 |
| With an Extra Quality Inspection Certificate |  |  |  |  |  |  |  |  |  | 7 |
| Acc. to Customers’S Request\*\* |  |  |  |  |  |  |  |  |  | X |