**P19**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **P19 -** | **XX** | | **X** | **X** |
| **Version:** | | |
| standard 00 | | |
| custom-made\* XX | | |
| **Language:** | | | |
| Polish | |  | P |
| English | |  | E |
| other\* | |  | X |
| **Acceptance tests:** | | | | |
| without extra quality requirements | |  |  | 0 |
| with an extra quality inspection certificate | |  |  | 1 |
| according to customer’s request\* | |  |  | X |

\* only after agreeing with the manufacturer

**Order example:**

The code: **P19 - 00E0** means:

P19 – temperature and humidity transducer of P19 type

00 – standard version E – Englsh version

0 – without extra quality requirements.